*) TWO-WAY PROFESSIONAL SPEAKER

1. 개요

본 기기는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

200W RMS power handling

124 dB max SPL

60 ~ 20000 Hz frequency range

90° x 70° constant directivity coverage angle

1 x 8" high power woofer

1 x 1.4" voice coil compression driver

High quality plywood cabinet

Steel front grille with clothing

Installation points available on rear, top and bottom panels

4 pole EUROBLOCK connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 124 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 70°

Directivity index Q	: 9

System Sensitivity	: 95 dB

Power section

Nominal Impedance	: 8 ohm

Power Handling	: 200 W RMS

Peak Power Handling	: 800 W PEAK

Recommended Amplifier	: 400 W

Protections	: Dynamic active mosfet

Crossover Frequencies	: 1800 Hz

Transducers

Compression Driver	: 1x1.0", 1.4" v.c

Woofer	: 8", 1.7" v.c

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

CE marking	: Yes

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 6 x M6, 4 x M8, 2 x M10

Grille	: Steel with clothing

Color	: Black - RAL 9005, White - RAL 9003

Size

Height	: 442 mm / 17.4 inches

Width	: 257 mm / 10.12 inches

Depth	: 284 mm / 11.18 inches

Weight	: 10.5 kg / 23.15 lbs

* COMPACT M 08 동급이상품