*) BASS REFLEX SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

400 W RMS power handling

124 dB max SPL

50 ÷ 200 Hz frequency range

1 x 10" high power woofer

High quality plywood cabinet

Steel front grille with clothing

M20 standard pole mount in top section of cabinet

4 pole EUROBLOCK connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 45 Hz ~ 200 Hz

Max SPL @ 1m	: 124 dB

System Sensitivity	: 92 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 400 W RMS

Peak Power Handling	: 1600 W PEAK

Recommended Amplifier	: DMA 162, DMA 162P, DMA 504, IPS 1.5K,	IPS 2.5K, QPS 6.0K

Transducers

Woofer	: 1 x 10", 2.5" v.c

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 12 x M10

Pole mount/Cap	: M20 thread

Grille	: Steel with clothing

Color	: Black

Size

Height	: 318 mm / 12.52 inches

Width	: 450 mm / 17.72 inches

Depth	: 360 mm / 14.17 inches

Weight	: 19.6 kg / 43.21 lbs

* S 10 동급이상품