*) BASS REFLEX SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

500W AES power handling

126 dB max SPL

35 ÷ 200 Hz frequency range

1 x 15" high-power woofer

High-quality plywood cabinet

Steel front grille with clothing

M20 standard pole mount in the top section of the cabinet

4 pole EUROBLOCK connector (audio input and parallel link output)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 35 Hz ~ 200 Hz

Max SPL @ 1m	: 126 dB

System Sensitivity	: 95 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 500 W RMS

Peak Power Handling	: 2000 W PEAK

Recommended Amplifier	: QPS 6.0K, IPS 2.5K, IPS 1.5K, DMA 504

Transducers

Woofer	: 1 x 15", 3.0" v.c

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Hardware	: 12 x M10

Pole mount/Cap	: M20 thread

Grille	: Steel with clothing

Color	: Black

Size

Height	: 443 mm / 17.44 inches

Width	: 630 mm / 24.8 inches

Depth	: 500 mm / 19.69 inches

Weight	: 27.5 kg / 60.63 lbs

* S 15 동급이상품