*) HIGH-EFFICIENCY SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

18" high-efficiency 4" voice-coil woofer with Inside/Outside Coil Technology

137 dB maximum sound pressure level

Response down to 30 Hz

Rectangular box enclosure with protective metal grille

35 mm standard pole mount in top section of cabinet

Baltic Birch cabinet painted with black, heavy duty, textured epoxy

Integrated hand carry points

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 30 Hz ~ 200 Hz

Max SPL @ 1m	: 137 dB

System Sensitivity	: 100 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 1500 W

Peak Power Handling	: 6000 W PEAK

Transducers

Woofer	: 18" neo, 4.0" v.c

Input/Output section

Input connectors	: Speakon NL4

Output connectors	: Speakon NL4

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Handles	: Integrated hand carry points

Pole mount/Cap	: M20 thread

Grille	: Metal

Color	: Black

Size

Height	: 639 mm / 25.16 inches

Width	: 530 mm / 20.87 inches

Depth	: 770 mm / 30.31 inches

Weight	: 43 kg / 94.8 lbs

* S 8018 II 동급이상품