*) BASS REFLEX SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 x 18" high-efficiency 4.0" voice-coil woofer with Inside/Outside Coil Technology

141 dB maximum sound pressure level

Response down to 30 Hz

System Power rating 3000 Watt RMS

M20 standard pole mount in top section of cabinet

Baltic Birch cabinet painted with black, heavy duty, textured epoxy

Recessed Speakon NL4 Input/Output

Protective metal grille, polyester fabric coated

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 30 Hz ~ 200 Hz

Max SPL @ 1m	: 141 dB

System Sensitivity	: 101 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 4 ohm

Power Handling	: 3000 W

Peak Power Handling	: 12000 W PEAK

Transducers

Woofer	: 2 x 18”, 4.0” v.c

Input/Output section

Input connectors	: Speakon NL4

Output connectors	: Speakon NL4

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Handles	: Integrated hand carry points

Pole mount/Cap	: M20 thread

Grille	: Metal

Color	: Black

Size

Height	: 639 mm / 25.16 inches

Width	: 1045 mm / 41.14 inches

Depth	: 770 mm / 30.31 inches

Weight	: 80 kg / 176.37 lbs

* S 8028 II 동급이상품