*) HIGH-POWER BASS REFLEX SUBWOOFER

1. 개요

본 기기는 저음역대 재생을 담당하는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Up to 3000 W power handling

143 dB max SPL

25 ÷ 200 Hz frequency range

2x19" HyperVented Neodymium Woofer with 4’’ v.c.

High-quality polyurea-coated multi-ply cabinet

Steel front grille with clothing

M20 standard pole mount in top section of cabinet

Speakon NL4 connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 25 Hz ~ 200 Hz

Max SPL @ 1m	: 143 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 4 ohm

Power Handling	: 3000 W

Peak Power Handling	: 12000 W PEAK

Woofer	: 2 x 19", 4.0" v.c

Input/Output section

Input connectors	: Speakon® NL4

Output connectors	: Speakon® NL4

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plywood

Handles	: 2 side

Pole mount/Cap	: M20 thread

Grille	: Steel with clothing

Size

Height	: 534 mm / 21.02 inches

Width	: 1300 mm / 51.18 inches

Depth	: 730 mm / 28.74 inches

Weight	: 85 kg / 187.39 lbs

* S 29 동급이상품