*) WEATHERPROOF LINE ARRAY MODULE

1. 개요

본 기기는 날씨 및 주변 환경에 영향을 받는 야외 설치에 적합한 2-way 라인 어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Very compact size

Maximum output per size available on the market

Wide, constant directivity, horizontal coverage angle

Minimum weight

Watertight multi-pole connector IP67

Baltic birch cabinet

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 55 Hz ~ 20000 Hz

Max SPL @ 1m	: 135 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 15°

Directivity index Q	: 16

Power section

Amplification	: Bi-Amp

Crossover Frequencies	: Recommended 800 Hz

Nominal Impedance LF	: 16 ohm

Power Handling LF	: 600 W

Peak Power Handling LF	: 2400 W

Sensitivity LF	: 98 dB

Nominal Impedance HF	: 16 ohm

Power Handling HF	: 110 W

Peak Power Handling HF	: 440 W

Sensitivity HF	: 109 dB

Transducers

Compression Driver	: 1 x 1.5", 3.0" v.c

Woofer	: 2 x 10", 2.5" v.c

Input/Output section

Input connectors	: Cable

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 6 x M10 inserts

Grille	: Steel with waterproof clothing

Color	: White, Black

Size

Height	: 334 mm / 13.15 inches

Width	: 735 mm / 28.94 inches

Depth	: 450 mm / 17.72 inches

Weight	: 30.2 kg / 66.58 lbs

* HL 20-WP 동급이상품