*) LONG THROW THREE-WAY SYSTEM

1. 개요

본 기기는 공연장, 경기장, 종교시설 등 중/대형 공간에 적합한 장거리 전송과 넓은 분산각도를 제공하는 3-way 바이앰프 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1000 W (LF) + 900 W (MHF) power handling

147 dB max SPL

43 ~ 18000 Hz frequency range

90° x 30° coverage angles

Fully equipped with neodymium transducers

Bi-amped system with passive filter between MF and HF

Horn Loaded symmetric design

Baltic birch plywood cabinet and steel grille

Weatherproof treatment

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 43 Hz ~ 18000 Hz

Frequency Response (-3dB)	: 59 Hz ~ 13000 Hz

Max SPL @ 1m	: 147 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 30°

Directivity index Q	: 12

Power section

Amplification	: Bi-Amp

Nominal Impedance LF	: 8 ohm

Power Handling LF	: 1000 W

Peak Power Handling LF	: 4000 W

Sensitivity LF	: 97 dB

Nominal Impedance MF+HF	: 8 ohm

Power Handling MF+HF	: 900 W

Peak Power Handling MF+HF	: 3600 W

Sensitivity MF + HF	: 111 dB

Protections MF+HF	: Dynamic Active Mosfet

Crossover Frequencies	: 1000 Hz

Transducers

Compression Driver	: 2 x 1.4" neo, 4.0" v.c

Midrange	: 2 x 10" neo, 3.0" v.c

Woofer	: 2 x 15" neo, 3.5" v.c

Input/Output section

Input connectors	: Screw Terminals

Output connectors	: Screw Terminals

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware

- n° 8 x M20 on each side panel

- n° 8 x M20 on top and bottom panels

Grille	: Steel

Color	: White - RAL 9010, Black - RAL 9005

Size

Height	: 525 mm / 20.67 inches

Width	: 1382 mm / 54.41 inches

Depth	: 815 mm / 32.09 inches

Weight	: 110 kg / 242.51 lbs

* HVL 15-L 동급이상품