*) THREE WAY INDOOR/OUTDOOR HORN LOADED SPEAKER SYSTEM

1. 개요

본 기기는 패시브 타입의 3-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

1300 W RMS power handling

136 dB max SPL

50 ~ 20000 Hz frequency range

Fully Horn-loaded, 60° x 40° directivity

15" neodymium woofer, 4.0" v.c.

10" neodymium midrange, 3.0" v.c.

3.0" v.c. neodymium compression driver

Active Mosfet Compression Driver Protection

Rotable HF Horn

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 50 Hz ~ 20000 Hz

Frequency Response (-3dB)	: 65 Hz ~ 20000 Hz

Max SPL @ 1m	: 136 dB

Horizontal coverage angle	: 60°

Vertical coverage angle	: 40°

Directivity index Q	: 12

Power section

Amplification	: Bi-Amp

Crossover Frequencies	: Recommended 300 Hz

Nominal Impedance LF	: 8 ohm

Power Handling LF	: 900 W

Peak Power Handling LF	: 3600 W

Sensitivity LF	: 100 dB

Nominal Impedance MF+HF	: 8 ohm

Power Handling MF+HF	: 400 W

Peak Power Handling MF+HF	: 1600 W

Sensitivity MF + HF	: 108 dB

Protections MF+HF	: Active mosfet compression driver

Crossover Frequencies	: 1300 Hz

Transducers

Compression Driver	: 1 x 1.4" neo, 3.0" v.c

Midrange	: 1 x 10" neo, 3.0" v.c

Woofer	: 1 x 15" neo, 4.0" v.c

Input/Output section

Input connectors	: Amphenol eco/mat IP 67

Output connectors	: Amphenol eco/mat IP 67

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 12 x M10 rigging point

Handles	: 2 recessed

Grille	: Steel

Color	: Black

Size

Height	: 890 mm / 35.04 inches

Width	: 519 mm / 20.43 inches

Depth	: 632 mm / 24.88 inches

Weight	: 52 kg / 114.64 lbs

* H 1315 WP 동급이상품