*) WEATHERPROOF TWO-WAY SPEAKER

1. 개요

본 기기는 날씨 및 주변 환경에 영향을 받는 야외 설치에 적합한 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

100 W RMS power handling

121 dB max SPL

80 Hz ÷ 20000 Hz frequency range

8" woofer, 1.5" v.c.

1.4" v.c. neodymium compression driver

90° x 60° constant directivity

Weatherproof IP55 cabinet with UV protection

Aluminum grille

Built in 100V line transformer

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 80 Hz ~ 20000 Hz

Max SPL @ 1m	: 121 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 60°

Directivity index Q	: 11

System Sensitivity	: 95 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 16 ohm

Power Handling	: 100 W

Peak Power Handling	: 400 W PEAK

Protections	: PTC

Crossover Frequencies	: 2200 Hz

Transducers

Compression Driver	: 1 x 1.0", 1.4" v.c

Woofer	: 1 x 8", 1.5" v.c

Input/Output section

Input connectors	: Neoprene Cable

Constant Voltage Transformer	: 100 V

Power selection 1	: 60 W - 167 ohm

Power selection 2	: 30 W - 333 ohm

Power selection 3	: 15 W - 667 ohm

Standard compliance

IP protection grade	: IP 55

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PE Low Density

Hardware	: 4 x M8 + U-bracket and pair of spacers

Grille	: Aluminum with waterproof clothing

Color	: Grey, White - RAL 9003

Size

Height	: 266 mm / 10.47 inches

Width	: 493 mm / 19.41 inches

Depth	: 250 mm / 9.84 inches

Weight	: 11.8 kg / 26.01 lbs

* P 1108T 동급이상품