*) WEATHERPROOF COAXIAL TWO-WAY SPEAKER

1. 개요

본 기기는 날씨 및 주변 환경에 영향을 받는 야외 설치에 적합한 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

600 W RMS power handling

134 dB max SPL

75 Hz ÷ 20000 Hz frequency range

15" neodymium woofer, 3.0" v.c.

2.5" v.c. neodymium compression driver

60° x 60° constant directivity

Weatherproof IP55 cabinet with UV protection

Aluminum grille

AISI 316L stainless steel bracket

12 suspension points (M10)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 75 Hz ~ 20000 Hz

Max SPL @ 1m	: 134 dB

Horizontal coverage angle	: 60°

Vertical coverage angle	: 60°

Directivity index Q	: 13

System Sensitivity	: 100 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 600 W

Peak Power Handling	: 2400 W PEAK

Protections	: Dynamic active mosfet

Crossover Frequencies	: 1100 Hz

Transducers

Compression Driver	: 1.3" neo, 2.5" v.c

Woofer	: Coaxial 15" neo, 3.0" v.c

Input/Output section

Input connectors	: Neoprene Cable

Standard compliance

IP protection grade	: IP 55

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PE Low Density

Hardware	: 12 x M10 + U-Bracket and Pair of spacers

Grille	: Aluminum with waterproof clothing

Color	: Grey, White - RAL 9003

Size

Height	: 463 mm / 18.23 inches

Width	: 463 mm / 18.23 inches

Depth	: 433 mm / 17.05 inches

Weight	: 17 kg / 37.48 lbs

* P 6215 동급이상품