*) WEATHERPROOF SUBWOOFER

1. 개요

본 기기는 날씨 및 주변 환경에 영향을 받는 야외 설치에 적합한 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

800 W RMS power handling

132 dB max SPL

50 Hz ÷ 200 Hz frequency range

15" neodymium woofer, 4.0" v.c.

Weatherproof IP55 cabinet with UV protection

Aluminum grille

AISI 316L stainless steel bracket

12 suspension points (M10)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 50 Hz ~ 200 Hz

Max SPL @ 1m	: 132 dB

System Sensitivity	: 97 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 8 ohm

Power Handling	: 800 W

Peak Power Handling	: 3200 W PEAK

Transducers

Woofer	: 15" neo, 4.0" v.c

Input/Output section

Input connectors	: Neoprene Cable

Standard compliance

IP protection grade	: IP 55

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: PE Low Density

Hardware	: 12 x M10 + U-Bracket and Pair of spacers

Grille	: Aluminum with waterproof clothing

Color	: Black

Size

Height	: 463 mm / 18.23 inches

Width	: 463 mm / 18.23 inches

Depth	: 433 mm / 17.05 inches

Weight	: 16.5 kg / 36.38 lbs

* P 8015S 동급이상품