*) TWO CHANNELS PROFESSIONAL POWER AMPLIFIER

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 2채널 파워 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 x 1250 W Class-H Power

Fast response and low distortion

Stereo, parallel, bridge modes

Extensive protection circuit

Variable speed cooling system

Signal, clip, fault led indicators

XLR input connectors

speakON and binding post output connectors

Limiter on each channel

3. 규격 및 사양

Amplifier specifications

Amplifier Class	: H

Output Power

- 2 x 1250 W @ 4 ohm

- 2 x 800 W @ 8 ohm

- 1 x 2500 W @ 8 ohm (bridge)

Frequency Response (-3dB)	: 20 Hz ~ 22000 Hz

Crosstalk	: <80 dB

Distortion (THD+N) @ 1 kHz nominal power	: <0.01 %

Input section

Total number of inputs	: 2

Balanced	: 2

Mono	: 2

Line inputs	: 2

Line connectors	: XLR

Output section

Signal output number	: 2

Signal output connectors	: XLR

Power output connectors	: Binding Post, Speakon

Configuration and control

Configuration	: DIP switch, Front panel

Protections

Cooling	: Forced

Short circuit	: Yes

Thermal	: Yes

DC	: Yes

Fuses	: Yes

VHF (Very High Frequencies)	: Yes

Power requirement

Operating voltage	: 220-240/115 V~ 50/60Hz

Power consumption	: 900 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Color	: Black-RAL9005

Rack mounting	: 19", 2U

Size

Height	: 88 mm / 3.46 inches

Width	: 482 mm / 18.98 inches

Depth	: 325 mm / 12.8 inches

Weight	: 11.2 kg / 24.69 lbs

* IPS 2.5K 동급이상품