*) FOUR CHANNELS PROFESSIONAL POWER AMPLIFIER

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 4채널 파워 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

4 x 2,500 W class HD power amplifier

Fast response and low distortion

Stereo, parallel and bridge modes

Comprehensive protection circuits

Variable speed cooling

Signal, clip, fault led indicators

XLR inputs and speakON outputs

Limiter on each channel

20 ~ 20000 Hz frequency range

3. 규격 및 사양

Amplifier specifications

Amplifier Class	: HD

Output Power

- 4 x 2500 W @ 2 ohm

- 4 x 2200 W @ 4 ohm

- 4 x 1400 W @ 8 ohm

- 2 x 5000 W @ 4 ohm (bridge)

- 2 x 4400 W @ 8 ohm (bridge)

Frequency Response (-3dB)	: 20 Hz ~ 20000 Hz

SNR Analog inputs (“A” weighted)	: >110 dB

Crosstalk	: <70 dB

Distortion (THD+N) @ 1 kHz nominal power	: <0.05 %

Input section

Total number of inputs	: 4

Balanced	: 4

Mono	: 4

Line inputs	: 4

Line connectors	: XLR

Output section

Signal output number	: 2

Signal output connectors	: XLR

Power output connectors	: Speakon

Protections

Cooling	: Forced

Short circuit	: Yes

Thermal	: Yes

DC	: Yes

Fuses	: Yes

VHF (Very High Frequencies)	: Yes

Power requirement

Operating voltage	: 220-240/115 V~ 50/60Hz

Power consumption	: 1900 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Handles	: Metal handles included in the front panel

Color	: Black - RAL 9005

Rack mounting	: 19", 2U

Size

Height	: 88 mm / 3.46 inches

Width	: 483 mm / 19.02 inches

Depth	: 399 mm / 15.71 inches

Weight	: 14.2 kg / 31.31 lbs

* QPS 10K 동급이상품