*) HIGH POWER AMPLIFIER

1. 개요

본 기기는 스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 4채널 파워 앰프로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Fast response and low distortion

Easy to configure in stereo / mono / bridge modes

Extensive protective circuits ensure high reliability and operating safety

Front panel signal / clippings / protection / temperature LEDs indicators

Minimum load impedance (stereo / mono): 2 Ohm

XLR input connectors

SPEAKON NL4 output connectors

Voltage clip switchable limiters

3. 규격 및 사양

Amplifier specifications

Output Power

- 4 x 2400 W @ 2 ohm

- 4 x 2200 W @ 4 ohm

- 4 x 1300 W @ 8 ohm

Frequency Response (-3dB)	: 20 Hz ~ 25 Hz

Distortion (THD+N) @ 1 kHz nominal power	: <0.1 %

Input section

Total number of inputs	: 4

Balanced	: 4

Mono	: 4

Line inputs	: 4

Line connectors	: XLR

Output section

Signal output number	: 2

Signal output connectors	: XLR

Power output connectors	: Speakon

Configuration and control

Configuration	: DIP switch, Front panel

Protections

Cooling	: Forced

Thermal	: Yes

DC	: Yes

Fuses	: Yes

VHF (Very High Frequencies)	: Yes

Power requirement

Operating voltage	: 220-240/115 V~ 50/60Hz

Power consumption	: 1950 W

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Metal

Rack mounting	: 19", 2U

Size

Height	: 88 mm / 3.46 inches

Width	: 482 mm / 18.98 inches

Depth	: 445 mm / 17.52 inches

Weight	: 16 kg / 35.27 lbs

* QPS 9600 동급이상품