*) 24-BIT 192kHz USB AUDIO INTERFACE

1. 개요

본 기기는 마이크, 악기 등을 연결하여 사용할 수 있는 2채널 오디오 인터페이스로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 In 2 Out USB 2.0 Bus-Powered Audio Interface

Up to 24-Bit/192kHz

2 Mic and Instrument/Line Combo input

High-Quality Preamps

Balanced Output

Independent Headphone Volume Control

Zero-latency monitoring

Independent Gain Control with Signal-Peak LED

Perfect for RDNet Measures

Rack Mount Ears included

3. 규격 및 사양

General specifications

MIC INPUT 1/2 (Balanced)

- Freq. Response	: 20Hz-20kHz, +/-0.1 dB

- THD+N	: <0.0011%, -1dBFS, 20Hz-20kHz	- Noise EIN	: < -120dB

- Dynamic Range	: 107dB (A-weighted)

- Input Impedance	: 3.5KOhm

- Gain Range	: -9 dB ~ +47 dB

- Maximum Input Level	: +9 dBu

LINE INPUT 1/2 (Balanced)

- Freq. Response	: 20Hz-20kHz, +/-0.1dB

- THD+N	: <0.0011%, -1dBFS, 20Hz ~ 20kHz

- Dynamic Range	: 107 dB (A-weighted)

- Input Impedance	: 15 kOhm

- Gain Range	: -20 dB ~ +36 dB

- Maximum Input Level	: +20 dB

INSTRUMENT INPUT 1/2 (Unbalanced)

- Freq.Response	: 20Hz-20kHz, +/-0.1dB

- THD+N	: <0.0025%, -1dBFS, 20Hz-20k

- Input Impedance	: 1MOhm

- Gain Range	: -10 dB ~+46 dB

- Maximum Input Level	: +10 dBu

- Dynamic Range	: 107 dB (A-weighted)

ANALOG OUTPUT (Balanced)

- Maximum Output Level	: 0dBFS=12dBu

- Freq.Response	: 20 Hz-20 kHz, +/-0.2

- THD+N	: <0.0012%, -1dBFS, 20 Hz-20 kHz

- Dynamic range	: 107 dB (A-weighted)

HEADPHONES OUTPUT (Unbalanced)

- Output Impedance	: <10 Ohm

- Max Output Level	: 500 Ohm - 114 mW

SUPPORTED SAMPLE RATES	: 44.1 kHz, 48 kHz, 88.2 kHz, 96 kHz,	176.4 kHz, 192 kHz

SUPPORTED BIT DEPTH	: 16 Bit, 24 Bit

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Steel

Hardware	: Rack mount ears incuded

Color	: Black - RAL 9005

Rack mounting	: 1/2 19", 1U

Size / Weight

Height	: 46 mm / 1.81 inches

Width	: 210 mm / 8.27 inches

Depth	: 125.8 mm / 4.95 inches

Weight	: 0.85 kg / 1.87 lbs

* TRK PRO2 동급이상품