*) TWO-WAY CEILING SPEAKER

1. 개요

본 기기는 천정에 설치 할 수 있는 2-way 실링 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

5" woofer with 1" dome tweeter

Power selectable (100 V): 30 W – 20 W – 10 W – 5 W

91 dB sensitivity

Colour white RAL 9016 and black RAL 9005

Self-extinguishing plastic frame and back can, steel grille

In/out euroblock connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 70 Hz ~ 20000 Hz

Max SPL @ 1m	: 112 dB

Coverage angle	: 120°

System Sensitivity	: 91 dB

Power section

Amplification	: Full Range

Nominal Impedance	: 16 ohm

Power Handling	: 60 W

Peak Power Handling	: 240 W PEAK

Crossover Frequencies	: 3000 Hz

Recommended Amplifiers	: DMA 504, DMA 162, DMA 82, DMA 162P,	ES 2160, ES 3080, AM 2320, AM 2160,	AM 2080, AM 1125, UP 8504, UP 8502,	UP 8501, UP 2321, UP 2162

Transducers

Dome Tweeter	: 1 x 1.0" neo

Woofer	: 1 x 6.0" neo

Input/Output section

Input connectors	: Euroblock

Output connectors	: Euroblock

Constant Voltage Transformer	: 100 V

Power selection 1	: 30 W - 333 ohm

Power selection 2	: 20 W - 500 ohm

Power selection 3	: 10 W - 1000 ohm

Power selection 4	: 5 W - 2000 ohm

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Plastic

Grille	: Steel

Color	: White - RAL 9016, Black - RAL 9005

Size

Depth	: 156 mm / 6.14 inches

Diameter	: 266 mm / 10.47 inches

Cut out diameter	: 245 mm / 9.65 inches

Weight	: 2.1 kg / 4.63 lbs

* MQ 50C 동급이상품