*) TWO-WAY PASSIVE WALL MOUNT SPEAKER

1. 개요

본 기기는 벽부에 설치 할 수 있는 패시브 타입의 2-way 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

2 x 3" full-range transducers with 1" dome tweeter

Power selectable (70 V / 100 V): 40 W – 20 W – 10 W – 5 W – 2.5 W

88 dB sensitivity

Colour black RAL 9005

Voice Alarm EN 54-24 Certified

In/out ceramic terminal block

Thermal fuse protection

Connections integrated in the wall support

UL rated plastic enclosure

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 80 Hz ~ 22000 Hz

Max SPL @ 1m	: 105 dB

Max SPL @ 4m	: 93 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 160°

System Sensitivity	: 88 dB

System Sensitivity 1W @ 4m	: 76 dB

Power section

Amplification	: Full Range

Nominal Impedance (ohm)	: 8 ohm

Power Handling	: 40 W

Peak Power Handling	: 160 W PEAK

Protections	: Thermal fuse - PTC

Crossover Frequencies	: 2500

Transducers

Dome Tweeter	: 1.0" neo, 1.0" v.c

Woofer	: 2 x 3.0", 1.0" v.c

Input/Output section

Input connectors	: Ceramic screw terminals

Output connectors	: Ceramic screw terminals

Constant Voltage Transformer	: 70/100 V

Power selection 1	: 40 W - 250 ohm

Power selection 2	: 20 W - 500 ohm

Power selection 3	: 10 W - 1000 ohm

Power selection 4	: 5 W - 2000 ohm

Power selection 5	: 2.5 W - 4000 ohm

Standard compliance

Safety agency	: CE compliant

EN54-24 certified	: Yes

CPR number	: 0068/CPR/057-2019

Physical specifications

Cabinet/Case Material	: ABS

Hardware	: Wall mount brackets

Grille	: Steel

Color	: Black - RAL 9005

Size

Height	: 399 mm / 15.71 inches

Width	: 92 mm / 3.62 inches

Depth	: 236 mm / 9.29 inches

Weight	: 5 kg / 11.02 lbs

* WMF 33EN 동급이상품