*) AES/EBU & DMX CABLE

1. 개요

본 제품은 AES/EBU & DMX 케이블로 다음과 같은 규격에 준한다.

2. 기능 및 특성

AES/EBU, DMX 연결, 높은 유연성

나선형의 구리 메쉬 스크린과 알루미늄 기화 천을 사용하여 매우 좋은 차폐 효과를 가짐

특별히 거친 외피 사용으로 매우 내구성이 큼

적용: 스캐너 네트워킹, 조명 시스템, 디지털 믹싱 콘솔, 실내외 설치, 디지털 앰프, DAT 레코더 등

3. 규격 및 사양

Properties	: OFC oxygen free copper

Signal transmission	: symmetrical

Construction	: (2LI2Y0,34mm²)(ST)DY

Jacket material	: PVC

Jacket Ø [mm]	: 6,20

Number of Channels (AES/EBU, DMX)	: 1

Inner conductor (AES/EBU, DMX)	: 2

Inner conductor (AES/EBU, DMX) [mm²]	: 0,34

Inner conductor Ø (AES/EBU, DMX) [mm]	: 0,66

AWG (AES/EBU, DMX)	: 22

Shielding	: Copper spiral shielding + aluminum	steamed fleece

Shielding factor [%]	: 100

Copper strands (AES/EBU, DMX)	: 19

Copper strand Ø (AES/EBU, DMX) [mm]	: 0,15

Conductor insulation material	: Foam / Skin-PE

Conductor insulation Ø [mm]	: 1,50

Weight per 1 m [g]	: 50

UV-resistant	: yes

Fire load per m [kWh]	: 0,17

Style variant	: round

Packing	: 100 m spool

Temperature min. [°C]	: -25

Temperature max. [°C]	: 70

Width [mm]	: 6,2

Height [mm]	: 6,2

* BINARY 234 AES／EBU 동급이상품