*) VIDEO CABLE

1. 개요

본 제품은 비디오 케이블로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Inner conductor of solid, oxygen-free copper(OFC Class 6N)

High shielding factor, triple or quad shielding, low transfer impedances

Gas-injected insulation, smoothed, heavy-duty AL/PT foil

Trouble-free digital signal transmission with SAT/broadband cable/terrestrial systems

Robust and flexible

Simple and easy mounting

3. 규격 및 사양

Properties	: OFC oxygen free copper

Jacket material	: PE

Jacket Ø [mm]	: 10.30

Jacket Ø (video) [mm]	: 10,30

Inner conductor (video)	: 1

Inner conductor Ø (video) [mm]	: 1,60

AWG (video)	: 14

Shielding	: AL foil + Cu mesh, tinned + 2nd AL foil

Conductor insulation material	: Foam / Skin-PE

Conductor insulation Ø [mm]	: 7,30

Weight per 1 m [g]	: 101

Fire load per m [kWh]	: 0,7

Style variant	: round

Packing	: 100 m

Packing	: 500 m

Temperature min. [°C]	: -25

Temperature max. [°C]	: 70

Width [mm]	: 10,3

[mm]	: 10,3

* ASTRAL-1.6/7.3 HD 동급이상품