*) CONTROL SERVER

1. 개요

본 기기는 네트워크를 기반으로 연결되어 DSP 시스템 하드웨어 및 프로그램을 제어 할 수 있는 기기이며 다음과 같은 규격에 준한다.

2. 규격 및 사양

Processor	: Intel® 64 Architecture Chipset

Ethernet Cable	: Standard CAT5e or CAT6, maximum	device-to-device length = 100 meters

Maximum Devices Per System	: 80 units per Site File

Maximum Stored Presets	: 1000

PERIPHERAL CONNECTIVITY

Ethernet	: Integrated Intel® 10/100/1000 Network	Connection

Wi-Fi	: IEEE 802.11a/b/g/n

USB	: Two Hi-Speed USB 2.0 ports

Wi-Fi

Chipset	: Atheros XSPAN family with SST3, with	increased link rate by 100% at short range,	50% at mid-range and 25% at long range

Type	: IEEE 802.11n compliant and backward	compatible with 802.11a/b/g

Power	: 19 dBm maximum output (per chain) /	22 dBm (aggregate)

Frequency	: Simultaneous dual-band 2.4 GHz and 5 GHz	with Dynamic Frequency Selection (DFS).	IEEE 802.11 b/g/n: 2.412-2.462 GHz.	IEEE 802.11a/n: 5.18-5.24 + 5.745-5.825 GHz	(US) 5.18-5.24 GHz (Europe ETSI).

Data Transfer Rates	: Up to 300 Mbps

Radio Data Rates	: Auto rate sensing

Enhancements	: Dual-band 2x2 spatial multiplexing, cyclic-delay	diversity (CDD), low-density parity check (LDPC),	maximum ratio combining (MRC), space time	block code (STBC) and Tx beamforming (TxBF)

Antennae	: Two RP-SMA (reverse-polarity SMA) auto	switching omni-directional antennae providing	1.5 dBi nominal gain at 2.4 GHz and 2.1 dBi	nominal at 5 GHz

International	: Multi-Country Roaming Supported (IEEE 802.1d	Global Harmonization Standard)

Modulation	: OFDM: BPSK, QPSK, 16-QAM, 64-QAM; DSSS;	DBPSK, DQPSK, CCK

Security	: 40-bit (also called 64-bit) and 128-bit WEP,	WPA-PSK, WPA2-PSK, and WPA/WPA2	Enterprise, IEEE 802.11i encryption

Number of Simultaneous Connections : 50

Space Required	: 208.3 x 228.6 x 43.7 mm

Electrical	: 12 VDC @ 2.5 A, 30W(max.)

* CONTROL SERVER 동급이상품