*) WALL PANEL

1. 개요

본 기기는 아날로그 입/출력 신호를 연결 할 수 있는 벽부형 판넬이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

One XLR female mic/line input

One XLR male line output

One programmable button

Two programmable RGB LEDs

Fits US and Euro single-gang wall boxes

3. 규격 및 사양

Power	: PoE IEEE 802.3af; 15.4 W Max

Sampling Rate	: 48 kHz, 96 kHz (configure in Dante Controller)

Input THD+N	: 0.003% (+15 dBu @ 1 kHz @ 0 dB gain)

Input Frequency Response	: +-0.2 dB; 20 Hz-20 kHz (+4 dBu @ 0 dB	gain)

Input Dynamic Range	: > 110 dB (A-weighted @ 0 dB gain)

Input Crosstalk	: -107 dB (+4 dBu @ 1 kHz @ 0 dB gain)

Maximum Input Level	: +23.5 dBu (1% THD @ 1 kHz @ 0 dB gain)

Input EIN	: <-127 dBu (150 Ohm source impedance,	22.4 kHz BW)

Input CMRR	: >50 dB (1 kHz @ 0 dB gain)

Input Impedance	: 2k Ohms balanced

Phantom Power	: +48 VDC @ 10 mA maximum

Input Latency	: 0.77 mS (Analog in to Dante Send)

Output THD+N	: 0.005% (-4 dBFS @ 1 kHz)

Output Frequency Response	: +/- 0.2 dB; 20 Hz–20 kHz (+4 dBu @ 0 dB	gain)

Output Dynamic Range	: > 110 dB (A-weighted @ 0 dB gain)

Maximum Output Level	: +23.5 dBu (1% THD+N @ 1 kHz)

Output Impedance	: 300 Ohms balanced

Output Latency	: 0.60 mS (Dante Send to Analog Out)

* xIO XLR 1x1 동급이상품