*) ZONE MIXING MANAGEMENT

1. 개요

본 기기는 존 믹싱, 페이징, 뮤직 매니지먼트 기능을 가진 제품으로 통합제어 시스템과 연동 가능한 제품이며 다음과 같은 규격에 준한다.

2. 규격 및 사양

Sample Rate	: 48 kHz

Frequency Response	: 20 Hz - 20 kHz, +/- 0.5 dB

Dynamic Range	: > 110 dB (A-Weighted), input to output

THD+Noise	: < -85 dB (un-weighted); 1 kHz @ +22 dBu	with 0 dB gain

Interchannel Crosstalk	: < -90 dB @ 1 kHz, typical

Latency	: < 1.6 ms, input to output with all DSP inactive

Space Required	: 480.2 x 221.5 x 43.7 mm

Electrical	: 100-240 VAC, 50/60 Hz, 25W(max.)

INPUTS

Number of Inputs	: Twelve (12) total; Four (4) switchable balanced	mic or line, Eight (8) mono-summed stereo -10	dBV line level

Connectors	: 3.81 mm terminal blocks (mic/line),	RCA (Audio Media source)

Nominal Input Level	: +4 dBu line or -36 dBu mic level (software	selectable) with 20 dB of headroom

Mic Pre-amp Gain	: +40 dB

Maximum Input Level	: +23 dBu mic/line, +8 dBV RCA

Input Impedance	: > 18 kΩ balanced, > 9 kΩ unbalanced,	> 2 kΩ with phantom power engaged Euroblock);	> 20 kΩ unbalanced (RCA)

CMRR	: > 50 dB @ 1 kHz, unity gain

Mic Pre-amp EIN	: < -125 dBu, 22 Hz - 22 kHz, 100 Ω source	impedance

Phantom Power	: +20 VDC, 20 mA maximum per input

OUTPUTS

Number of Outputs	: Six (6) balanced line level

Connectors	: 3.81 mm terminal blocks

Nominal Output Level	: +4 dBu line level with 20 dB of headroom.	For unbalanced analog output, do not connect	the minus output terminal.	Unbalanced configuration results in 6 dB lower	output level.

Maximum Output Level	: +24 dBu

Output Impedance	: 200 Ω balanced, 100 Ω unbalanced

* ZONE MIX 761 동급이상품