*) DSP SYSTEM

1. 개요

본 기기는 건물, 공연장 등 대규모 시스템 구성에 적합한 디지털 시그널 프로세서로 오디오 네트워크, AEC 등 다양한 기능을 제공하며 다음과 같은 규격에 준한다.

2. 기능 및 특성

256 x 256 Dante I/O channels, option to add 128 x 128 Dante I/O channel

64 channels of acoustic echo cancellation (AEC), option to add 32 AEC channels

32 media playback channels, option to add 32 or 96 media playback channels

8 media record channels

Lua scripting support standard

Third-party control via Intelligent Modules

3. 규격 및 사양

Operating System	: Linux based built for purpose

Audio Engine	: Updated premium performance at 48kHZ	sampling rate

Dante	: 256 x 256 I/O channels

AEC	: 64 channels of acoustic echo cancellation at	256 ms tail length with the latest algorithms

Media playback channels	: 32

Media record channels	: 8

DSP Management	: Composer Windows application manages all	aspects of audio, control, and security

Third-Party Control	: Expanded Intelligent Modules for controlling	various types of devices

Programming	: Support for Lua scripting

Embedded Web Server	: Provides remote metering, diagnostics, and	configurable ARC-WEB browser-based control

IT Device Management	: HPE ILO (Integrated Lights Out)

Platform	: HPE ProLiant DL20 Gen11

Processing	: Multi-core server class CPU

System Storage Drive	: 500 GB SSD

Media Storage Drive	: 500 GB SSD for record and playback

Dante Networking	: 2x RJ45 1 Gbit/Sec

Control Networking	: 1x RJ45 1 Gbit/Sec

Management	: 1x RJ45 ILO port with SNMP support

Form Factor	: 1 RU rack mountable

Dimensions	: 43.2 x 434.6 x 382.2 mm

* Server D100 동급이상품