*) THREE-WAY LINE ARRAY SPEAKER

1. 개요

본 기기는 라인어레이 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

148 dB max SPL

4 x 6” neo midrange drivers, 2” v.c.

2 x 1.4” neo compression drivers, 3” v.c.

2 x 12” neo woofers, 3.5” v.c.

90° x 10° 4PATH waveguide

Designed to operate with XPS 16K amplifier (3 modules per amp unit)

Durable and lightweight cabinet construction, polyurea coating

Heavy duty, powder coated, custom perforated front grille

2 x P-COM 8 pole bayonet connectors (Gold-plated, CA-COM compatible, IP 68)y

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 35 Hz - 20 kHz

Max SPL @ 1m	: 148 dB

Horizontal coverage angle	: 90°

Vertical coverage angle	: 10°

Power section

Amplification	: Quad-amp

Nominal Impedance LF	: 8 ohm

Nominal Impedance LF2	: 8 ohm

Nominal Impedance MF	: 8 ohm

Nominal Impedance HF	: 16 ohm

Transducers

Compression Driver	: 2 x 1.4” neo, 3” v.c.

Midrange	: 4 x 6.5” neo, 2” v.c.

Woofer	: 2 x 12” neo, 3.5” v.c.

Input/Output section

Input connectors	: P-COM 8POLE

Output connectors	: P-COM 8POLE

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Birch plywood

Hardware	: Array fittings

Handles	: 1 x side, 2 rear

Grille	: Steel with clothing

Color	: Black

Size

Height	: 366 mm / 14.41 inches

Width	: 1177.5 mm / 46.36 inches

Depth	: 540.6 mm / 21.28 inches

Weight	: 64.2 kg / 141.54 lbs

Shipping information

Height	: 605 mm / 23.82 inches

Width	: 1210 mm / 47.64 inches

Depth	: 400 mm / 15.75 inches

Weight	: 71.2 kg / 156.97 lbs

* GTX 12 동급이상품