*) 4K DECODER

1. 개요

본 기기는 네트워크 신호를 통해 비디오, 오디오 신호를 전송 할 수 있는 장비이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

A single Gigabit LAN Port for PoE Power, 4K UHD  Video, Audio, and Control

Easy Control Integration

Ultra-low Latency [ ~1 frame - visually lossless ]

Low bitrates

No fiber or 10 Gigabit switch required

Low-Cost network switches are used

Scalable / Unlimited Distribution

Any number and combination of inputs/outputs [in increments of one]

Standard network cabling [CAT5e/6]

Utilize existing network resources

Rapid deployment

Single network for AV and IT

Reduced operating costs

3. 규격 및 사양

Video Codec	: JPEG2000 based visually lossless video	compression algorithm

Audio Codec	: LPCM

Bit Rates	: 50 to 800 Mbps

Latency

- Ultra-low Latency (visually lossless video)

- 17ms @ 1080p60 & 4K60 4:2:0

- 33ms @ 4K30 4:4:4

Streaming Protocols	: IP, UDP, ICMP, IGMP

Copy Protection	: HDCP 2.2, AES-128 Encryption

Video

- Output	: 1x HDMI capable of scaling and outputting	video formats up to 4k30 4:4:4

Audio

- Output	: 1 digital audio output via HDMI

: 1 Analog Stereo Audio balanced output

Ethernet	: Network connectivity for control AV traffic

USB	: USB 2.0 host or device signal extension and	routing

Serial / RS-232	: Bi-directional device control and monitoring

HDMI	: HDCP 2.2, CEC

Connectors

- LAN	: 8-pin RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet port / PD port	: POE (IEEE 802.3af or 802.3at)

- HDMI OUTPUT	: HDMI Type A connector, female; HDMI digital	video/audio inputs

- 4 pin Euroblock 3.81mm pitch connector	: Stereo Unbalanced Analog Audio Input

- 5 pin Euroblock 3.81mm pitch connector	: RS-232 over IP

- USB Host	: (2) USB Type-A connector

Dimensions	(WxHxD)	: 146 x 29.3 x 136.4 mm

Weight	: 0.45 kg

* D4100 동급이상품