*) 4K WALLPLATE ENCODER

1. 개요

본 기기는 네트워크 신호를 통해 비디오, 오디오 신호를 전송 할 수 있는 벽부형 판넬이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

A single Gigabit LAN Port for PoE Power, 4K UHD Video, Dante®/AES67, and Control

Secure Network Isolation - VLAN Tagging separates AV trac on the corporate network

Easy installation in a wall, oor, or lectern

Mounts into standard Decora style wallplates

Easy Control Integration

Ultra-low Latency [ ~1 frame - visually lossless ]

Low bitrates

No ber or 10 Gigabit switch required

Low-Cost network switches are used

Scalable / Unlimited Distribution

Any number and combination of inputs/outputs [in increments of one]

Standard network cabling [CAT5e/6]

Utilize existing network resources

Rapid deployment

Single network for AV and IT

Reduced operating costs

3. 규격 및 사양

Video Codec	: JPEG2000 based visually lossless video	compression algorithm

Audio Codec	: DANTE®, AES67

Bit Rates	: 50 to 800 Mbps

Latency

- Ultra-low Latency (visually lossless video)

- 17ms @ 1080p60 & 4K60 4:2:0

- 33ms @ 4K30 4:4:4

Streaming Protocols	: IP, UDP, TCP, ICMP, IGMP

Copy Protection	: HDCP 2.2, AES-128 Encryption

Video

- Input	: 1x HDMI capable of receiving source input	video formats up to 4K60 4:2:0

Audio

- Input	: 1 digital input de-embedded from HDMI

: 1 Dante®/AES67 digital audio input	(up to 4 ch)

: 1 analog stereo input, unbalanced

- Output	: 1 analog stereo audio output (balanced)

: 1 Dante®/AES67 digital audio output	(up to 2 ch)

HDMI	: HDCP 2.2, EDID

Connectors

- LAN	: 8-pin RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet port / PD port

POE (IEEE 802.3af)

- HDMI INPUT	: (1) HDMI Type A connector, female; HDMI	digital video/audio inputs

- 3.5mm Barrel	: Analog Stereo Output (balanced),	Analog Stereo Output (unbalanced), IR over IP	Input, IR over IP Output, RS232 over IP

Dimensions	(WxHxD)	: 91.8 x 103.4 x 50.6 mm

Weight	: 0.45 kg

* DuetE-WP 동급이상품