*) IP MULTIVIEWER

1. 개요

본 기기는 다양한 비디오 소스를 한 화면에 표출시켜 주는 멀티 뷰어이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

Locate Anywhere on the Network . PacketAV™ stream inputs and outputs mean the MV4 does not have to be located near the sources or the displays, which often have space limitations

Easy Control Integration

Ultra-low latency

Low bitrates

No fiber or 10 Gigabit switch required

Low-Cost network switches are used

Scalable / Unlimited Distribution

Standard network cabling [CAT5e/6]

Utilize existing network resources

Rapid deployment

Single network for AV and IT

Reduced operating costs

3. 규격 및 사양

Video Codec	: JPEG2000 based visually lossless video	compression algorithm

Bit Rates	: 50 to 800 Mbps

Latency

- Ultra-Low Latency (visually lossless video)

- 42ms @ 1080p60

- 116ms @ 4K30 4:4:4

Streaming Protocols	: IP, UDP, TCP, ICMP, IGMP

Copy Protection	: HDCP 2.2, AES-128 Encryption

Video

- Input	: Up to (4) AV over IP streams from PacketAV	Matrix Series Ultra-Low latency 4K encoders over	Ethernet

- Output	: 1x HDMI capable of scaling and outputting	video formats up to 4K30 4:4:4

: 1x AV over IP stream over Ethernet

Audio

- Input	: Embedded in the AV over IP stream from the	PacketAV Matrix series encoder source.

- Output	: 1 Embedded AV over IP stream output.

: 1 digital audio output via HDMI

Front Panel Buttons	: Control via buttons along with	on-screen (OSD) Graphical User Interface

IP Control	: UDP Unicast / Multicast API Control (encoder	LAN port)

Connectors

- LAN1-4 (Decoder)	: 8-pin RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet ports

- LAN (Encoder)	: RJ-45 connector, female; 100BASE-TX /	1000BASE-T Ethernet port

- HDMI OUTPUT	: HDMI Type A connector, female; HDMI digital

video/audio inputs

- POWER	: One 120 Volt AC power input

Dimensions	(WxHxD)	: 431.8 x 44.2 x 191 mm

Weight	: 2.6 kg

* MV4 동급이상품