*) 16 CHANNEL ULTRA-WIDEBAND WIRELESS RACK

1. 개요

본 기기는 무선 마이크 시스템의 수신기 모듈을 장착 할 수 있는 장비로 다음과 같은 규격에 준한다.

2. 규격 및 사양

Frequency ranges	: 470 - 1260 MHz (full range)

Filter selection (10 automatically selected band-pass filters)	: 470-608 MHz / 470-694 MHz / 470-832 MHz	/ 470-1260 MHz / 510-608 MHz / 510-694 MHz	/ 510-832 MHz / 510-1260 MHz /	822-1260 MHz / 940-1260 MHz

Antenna connector	: 4 x BNC type female connectors for inputs,	2 x SMA type female connectors for loop

Antenna input impedance	: 50 Ohm

Spurious emissions	: < 2 nW

Input/output gain	: 1dB ± 1

Input/cascade gain	: 1dB ± 1

IP3	: 14 dBm

Antenna booster powering	: +12 Vcc / 300 mA MAX

Analogue audio output	: 2 x DB25 connectors (TASCAM)

Digital audio output	: AES59 (DB25 connector) and AES72 1M	(2 RJ45 connectors)

Dante output	: Dante Primary and Secondary (2 x 1000 Base	TX RJ45 Ethernet)

Monitor output	: headphone 6.3 mm jack socket, volume	adjustable with a front knob

LED

- 4 LEDs indication for the zone activation status (red, green, off)

- 4 LEDs indication for the booster status (red, green, off)

- 4 LEDs indication for the power supply status (red, green, blue, off)

- 1 LED indication for the MRK16 status (green, off)

Max number of receiver slots	: 4

Max number of channels	: 16 (with QUAD CHANNELS RECEIVER),	8 (with DUAL CHANNELS RECEIVER)

Managing interface	: 2 x 1000 Base TX RJ45 Ethernet, Remote	Control Interface, USB-C with powering 3A@5V	(optional) and thru display menu of the 1st	receiver on the right

Dimensions	: 44 x 483 x 352 mm

Weight	: 4.3 kg

* MRK16 동급이상품