*) DUAL WIDEBAND TRANSMITTER

1. 개요

본 기기는 무선 마이크 시스템 송신기로 다음과 같은 규격에 준한다.

2. 규격 및 사양

Frequency ranges	: from 430 to 1260 Mhz, depends on the country

Switchable channels	: 2400 managed in 40 groups ofr 60 channels	completely user customizable

Switching-window	: 330 MHz tuneable

Frequencies	: 5 kHz steps

RF Power	: switchable typ. 10,20,30,50,75,100,150,200,250,	400,500,750,1000,1200,1500,2000 mW (ERP)

Max RF output power	: 2 Watt

Antenna connector	: 2 x BNC type female connectors

Auxiliary RF connector	: 2 x SMA type female connectors

RF impedance	: 50 Ω

Modulation	: FM, MPX Stereo or mono, selectable with	dedicated menu

Peak deviation	: ±56 kHz for mono wideband, ±35 kHz for	mono narrowband, ±48 kHz for stereo (preset	mode)

MPX Pilot tone	: 19kHz

Tone squelch

- 32.789Hz (for Wisycom wireless microphone)

- 131,8 (for Wisycom intercom, i.e. NR)

Spurious emissions	: < 2 nW

AF bandwidth

- 20 ~ 20kHz (mono)

- 30 ~ 15kHz (stereo)

Audio input connector	: XLR-3 / 1/4“ (6,3mm) jack combo socket,	electronically balanced

Audio input level	: +18dBu

Pin Assignments

- XLR: 1=ground 2=hot 3 =cold

- 6.35mm (1/4“) TRS: Tip=hot Ring=cold Sleeve=ground

Digital output	: AES3 on XLR-3M (32kHz ~ 108 kHz)

Monitor output	: 6.35mm (1/4“) jack socket, balanced

Monitor output level	: 120+120mW@24Ω, 80+80mW@150Ω

Monitor out impedance	: 25Ω for auricle

Managing interface	: 10/100 Base TX Ethernet port on RJ45	connector, Bluetooth Long Range

Display	: 64 x 256 OLED (white)

Dimensions	: 43.8 x 483 x 349 mm with brackets

Weight	: 4 kg approx.

* MTK982 동급이상품