*) SMART PASSIVE WIDEBAND COMBINER

1. 개요

본 기기는 광대역 액티브 안테나 결합기/분할기로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Wideband: 170-1260 MHz

High Rf robustness and linearity: for high density/equally spaced frequencies operations (i.e. with MTP40s Linear)

Able to feed 8 diversity receivers

Combine/Select signal from 4 antenna inputs

Redundant DC supply and antennas diagnostic features

Wisycom Remote Antenna Protocol to control antennas/booster remotely thru coax

Ethernet interface to access all of feature with a PC, making presets and real time monitoring

Cascade output to connect another SPL2208 or monitor devices

3. 규격 및 사양

Frequency ranges	:170 ÷ 1260 MHz

Input/output gain	: +5dB approx.

Input/cascade gain	: +1.5dB approx.

Amplifier linearity	: ± 1 dB (typical)

Noise figure	: 7,5 dB

Antenna booster powering	: +12Vcc / 500mA MAX (for each BNC-female	input connector A & B)

Connector	: input 2+2 BNC-F

: output 8+8 BNC-F (SPL2208)

: cascade: 2 BNC-F

Impedance	: 50 Ω

Managing interface	: 10/100 Base TX Ethernet port and thru frontal	tactile buttons

Power supply	: 10÷ 28 Vdc, 5A max, redundant DC Vdc1 and	Vdc2 on XLR M-4pin

Power consumption	: 40W max

Temperature range	: -25 ÷ +55 °C

Material	: aluminum

Finishing	: black varnish

Dimensions	: 44 x 483 x 351 mm (HxWxD)

Weight	: 3 kg

* SPL2208 동급이상품