*) SMART PASSIVE WIDEBAND COMBINER

1. 개요

본 기기는 패시브 광대역 컴바이너로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Selectable combination thru a 2 positions selector on front panel [16:1] or 2x [8:1]

Used with MTK982/MTK952N permits to recover the combiner loss

Wide band operation 400÷1300MHz

High input power up to 2.5W

3. 규격 및 사양

Frequency ranges	: 400 ÷ 1300 MHz

Splitter/Combiner loss	: approx. 10 dB for 2x [8:1]	approx. 13dB for [16:1]

Max Input power	: 2.5W (for each input connector)

Connector input	: 16 BNC-F

output	: 3 BNC-F

Impedance	: 50 Ω

Managing interface	: selector in the front panel

Power supply	: Hirose 4pin connector, 10-28V 0.1A max

Temperature range	: -25 ÷ +55 °C

Material	: aluminum

Finishing	: black varnish

Dimensions	: 43,8 x 483 x 349 mm (HxWxD)

Weight	: 3,2 Kg

* CSI16T2 동급이상품