*) UHF ANTENNA

1. 개요

본 기기는 무선 마이크 시스템의 안테나이며 다음과 같은 규격에 준한다.

2. 기능 및 특성

Antenna & amplifier integrated in a single device

designed to amplifier RF signal up to 250 mW

powered by the transmitter or MFL system through the coaxial cable

housing is in ruggedized aluminum, with waterproof sealing (for version with N connector), suitable for outdoor installations

3. 규격 및 사양

Frequency range	: up 700 MHz (LxP-L), up 800 MHz (LxP-H), up	960 MHz (LxP-X), up 1300 MHz (LxP-W)

Max input power	: 4 dBm

Input/output impedance	: 50 ohm (SWR = < 1:1.2).

Connectors	: BNC-female type or N-female type (option CN)

Gain (max)	: 20 dB (typical)

OIP3	: +42 dBm (Output 3° order Intercept Point)	typical @ 27dBm - 1dB compression point

Powering	: +12 V, 200 mA (thru input coax. cable)

Dimension	: 276 x 336 x 61 mm (HxWxD)

Material	: Epoxy fiberglass (copper –clad)

Connector	: BNC type (for LBP), N type (for LNP)

Finishing	: Black matte

Mounting	: 5/8” Withworth or 3/8” with adapter

Weight	: 700g (LBP), 750g (LNP)

* LBP 동급이상품