*) SUBWOOFER SPEAKER

1. 개요

본 기기는 서브우퍼 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

144 dB max SPL

2 x 19” neo woofers, 4” v.c.

3 side handles

Designed to operate with XPS 16K amplifier (4 modules per amp unit)

Durable and lightweight cabinet construction, polyurea coating

Heavy duty, powder coated, custom perforated front grille

2 x 2 P-COM 8 pole bayonet connectors (Gold coated, CA-COM compatible, IP 68)

3. 규격 및 사양

Acoustical specifications

Frequency Response (-10dB)	: 25 Hz ÷ 200 Hz

Max SPL @ 1m	: 144 dB

Power section

Amplification	: Full Range

Nominal Impedance LF	: 8 ohm

Nominal Impedance LF2	: 8 ohm

Transducers

Woofer	: 2 x 19” neo, 4” v.c.

Input/Output section

Input connectors	: P-COM 8POLE

Output connectors	: P-COM 8POLE

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Birch plywood

Hardware	: Suspension Fittings, M20 Socket

Handles	: 3 x side

Grille	: Steel with clothing

Color	: Black

Size

Height	: 531.5 mm / 20.93 inches

Width	: 1310 mm / 51.57 inches

Depth	: 735 mm / 28.94 inches

Weight	: 96 kg / 211.64 lbs

Shipping

information Height	: 620 mm / 24.41 inches

Width	: 1360 mm / 53.54 inches

Depth	: 800 mm / 31.5 inches

Weight	: 102 kg / 224.87 lbs

* GTS 29 동급이상품