*) CD/MEDIA PLAYER

1. 개요

본 기기는 CD, USB 등을 연결하여 음원 소스를 재생하는 플레이어로 다음과 같은 규격에 준한다.

2. 기능 및 특성

Plays audio from CD, USB and 3.5mm sources

Super-fast loading, slot-in CD drive

10-key direct track access buttons

Random, Repeat, and Power-on-Play modes

Tempo control for fitness applications

Balanced XLR and unbalanced RCA line outputs

1RU rack-mountable

IR remote included

3. 규격 및 사양

Playable Formats / File Systems

- CD	: CD-DA (CD-TEXT), CD-ROM (ISO9660),	CD-R, MP3-CD

- USB	: FAT16 / FAT32

MP3 Format Supported

- Extension	: MP3

- Bitrate	: 32 to 320 kbps and VBR

- Sampling Frequency	: 44.1 kHz\16-bit

Tempo control

- Tempo range from	: -15% to +15%

- Tempo lock feature

Number of Channels	: 2 (stereo), 1 (mono)

Frequency Response	: 20 Hz - 20 kHz (± 1.0dB)

S/N Ratio	: > 95 dB (A-Weighted)

Total Harmonic Distortion (THD)	: < 0.01%

Dynamic Range	: > 85 dB

Channel Separation	: > 80 dB

Input

- Aux in	: TRS (3.5mm)

- Maximum input level	: 1 Vrms

Output

- Balanced XLR / unbalanced RCA

- Maximum output level	: 3 Vrms

USB Thumbdrive Specs

- Max storage capacity	: Up to 32 GB

- Max file size	: 2 GB

Power consumption	: 30W

Dimensions	: 434 x 347 x 44 mm

Weight	: 3.6kg

* DN-300C MKII 동급이상품