*) DIGITAL RACK MIXER

1. 개요

본 기기는 디지털 오디오 믹서로 다음과 같은 규격에 준한다.

2. 기능 및 특성

40-input channel, 25-bus, 1U rackmountable digital mixing core for live and installed sound application

25 time-aligned and phase-coherent mix buses

AES50 networking allows up to 96 inputs and 96 outputs

Open architecture allows for future 96 kHz operation

High-performance aluminium and high-impact steel structure

40 bit fl oating point digital signal processing

8 DCA and 6 mute groups

8 digital signal processing eff ects engines

32 x 32 channel USB 2.0 audio interface

Built-in expansion port for audio interface cards or digital networking bridges

MIDI In/Out for remote scene recall or controlling other MIDI equipment

DAW remote control emulations of Mackie Control* and HUI* protocols

Optional wireless remote control with MIDAS Apps for iPhone* and iPad*

Auto-ranging universal switch-mode power supply

3. 규격 및 사양

Processing

Number of processing channels	: 32 input channels, 8 aux channels, 8 FX return	channels, 16 aux buses, 6 matrices, main LRC

Internal effects engines, true stereo / mono	: 8 / 16

Internal total recall scenes (incl. preamp and fader)	: 100

Signal processing	: 40-bit floating point

Network I/O latency (stagebox in > console	processing* > stagebox out)	: 1.1 ms

Connectors

Talkback mic input, TRS	: 1 external (no phantom power)

Monitoring outputs ¼" TRS balanced : 2

AES50 ports, SuperMAC	: 2

Expansion card slot	: 32 channel audio input/output, various	standards

P-16 connector, ULTRANET (no power supplied)	: 1

MIDI inputs / outputs	: 1/1

Ethernet, RJ45, rear panel, for remote control	: 1

USB Type A, front panel, for audio and data export/import	: 1

Indicators

LCD screen	: 128 x 64, LCD with RGB color backlight

Status LEDs	: AES50 port A/B status, power LED, Mute All	button

Power

Switch-mode power supply Autorange	: 100-240 V (50/60 Hz)

Power consumption	: 40 W

Physical

Standard Operating Temperature Range	: 5°C – 40°C (41°F – 104°F)

Dimensions	: 483 x 300 x 50 mm

Weight	: 3.5 kg

* M32C 동급이상품.